3. Write an assembly language program for adding two 16-bit data using 8086 processor

PROGRAM:

LHLD 2050

XCHG

LHLD 2052

DAD D

SHLD 2055

HLT

OUTPUT:

